# Add Facing...

## S U

Keyboard Shortcut!

This feature is primarily a Sewer’s feature. You can add a facing to any outer seam on the garment.

To create a facing:

- Select one or more segments

- On the Additions menu, click Add Facing.

- When the dialog window appears, type in the name of the piece and its width.

- Click OK. The facing will appear.

Now, try selecting the neckline, shoulder and armhole and then request the facing command. You will create a one-piece facing as shown in the illustrations below.

Note:

The facing piece cannot be separated from the main garment in this version. We hope to do this in future versions, but for now, you will need to print the designated facing page a second time for the facing pattern.

Try selecting the neckline, shoulder and armhole and then request the facing command. You will get a one piece facing as shown in the illustrations below.